**Can't get the model down**

Seeing that the 3D printing finished product is done, but it is too tight to pull it off the platform. I feel the platform is being pulled off by me. This is because the high temperature of the machine's printing space, which should allow the machine's printing space to cool for a few minutes before using the configured tools and then remove it. It is also suggested that if the platform can be heated, the temperature of the platform can be adjusted to between 50 and 70 degrees. After heating for three minutes or so, and the model will be easily taken off. Note: If the forced removal of the finished product after printing, May cause deformation of the finished product or burns. Hand rubbing will damage the accuracy of the platform.